




Startup Responses







Startup Responses


Removing Lid







Steady State







Lid Sitting on Tray, No Screws






After Merge Confirmation






Lid Resting on top, no screws. Accel fit MA % rises to above 10 quickly



Unscrewing Lid. Happens at around 1.5seconds



Program sees instability, and that voltage is above a safe zone (700mV in this trial).

The voltage is immediately dropped to a safe level for no lid (600mV in this trial).

